**NAME................................................................................ ADM NO................ CLASS................**

**441/2**

**HOMESCIENCE (CLOTHING CONSTRUCTION)**

**FORM 4**

**PAPER 2 (PRACTICAL)**

**FORM 4 JANUARY 2023 TERM 1 OPENER EXAM**

**TIME 2 ½ HOURS**

A pattern of a girl’s skirt is provided. You are advised to study the sketches, instructions and layout carefully before you begin the test.

**Materials provided**

1. Pattern pieces

A – skirt back

B – skirt front

C – pocket

D – waistband

1. Plain light weight cotton fabric 55x90cm wide
2. Sewing thread to match the fabric
3. One large envelope.

**The test**

Using the materials provided, cut out and make the RIGHT HALF of the skirt to show the following processes.

1. Making of the back dart
2. Preparation of pleats on the skirt front.
3. Attachment of front pocket to the skirt front and back pocket to the skirt back. Do not trim or neaten the seam.
4. Making the side sea using an open seam. **Neaten below the pocket only.**
5. Joining of the pocket seam. **Do not neaten.**
6. Preparation of an interfaced waistband. (6mks)
7. Attachment of the waistband, **slip-hem the back piece only.**
8. Making of the worked loop on the back waistband for a 1cm wide button.

At the end of the examination, firmly sew onto your work, on a single fabric, a label bearing your name and index number. Remove needles and pins from your work, fold your work neatly and place it in the envelope provided. Do not put scraps of fabric in the envelope.

